|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | |  | | |  | | |  |  | |  | | | |  |  |  |  | | --- | --- | --- | --- | | **C-GHUF Summary View** | | | | | Registration | C-GHUF | Date | Sep 8, 2022 | | Make | BELL HELICOPTERS | TTAF | 19859.00 | | Model | 205A-1 | Serial No. | 30106 | | |  |  | | --- | --- | | **Actions** | | | Cal - Calibration | Ins - Inspection | | Ins - Inspection/Regrease | On - On Condition | | Ove - Overhaul | Per - Performance Test | | Rec - Recertification | Rep - Replacement | | Ret - Retirement | Ser - Service | |  |  | |

| **Cycles values** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Cycle Name** | **Value** | **Cycle Name** | **Value** | **Cycle Name** | **Value** | **Cycle Name** | **Value** |
| COMP | 18 959.0 | GP | 23 081.0 | HOBBS | 19 859.0 | HOOK TIME | 609.0 |
| IMP | 12 439.0 | Landings | 41 468.0 | LIFTS | 17 600.0 | PT | 7 728.0 |
| RIN | 59 068.0 | RIN-X2 | 153 336.0 | RIN-X5 | 383 340.0 | STARTS | 12 524.0 |

| **Components** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Battery / On  2430 | RG380E44 | 40606262 |  | 16669.20H Jun 10, 14 |  |  | 3189.80H 98.93M |  |  |
| Battery / On  2430 | RG380E44 | 40966663 |  | 18709.10H Mar 23, 19 |  |  | 1149.90H 41.50M |  |  |
| **ELT Operational Check / Rec 2560** | **S1840501-01** | **2620138-0022** | **12.00M\*** | **19677.50H Apr 12, 22 \*** | **\*** | **Feb 15, 23 \*** | **181.50H 4.87M\*** | **\*** | **5.23M\*** |
| *‣ ELT Battery / Rep 2560* |  |  | *72.00M\** | *19677.50H Apr 11, 22 \** | *\** | *Sep 1, 27 \** | *181.50H 4.90M\** | *\** | *59.77M\** |
| ELT Performance Check (Cabin) / Per 2560 |  |  | 24.00M\* | Apr 12, 22 \* | \* | Feb 15, 23 \* | 4.87M\* | \* | 5.23M\* |
| First Aid Kit / Ins 2560 | F891N270 | 31212 | 12.00M | 19783.10H Aug 1, 22 | 0.00 | Aug 31, 23 | 75.90H 1.23M |  | 11.77M |
| First Aid Kit / Ins 2560 | F891N270 | 31211 | 12.00M | 19783.10H Aug 1, 22 | 0.00 | Aug 31, 23 | 75.90H 1.23M |  | 11.77M |
| Survival Kit / Ove 2560 | FE7A | A514-3507 | 24.00M | 19790.10H Aug 5, 22 | 0.00H | Aug 5, 24 | 68.90H 1.10M |  | 22.90M |
| Survival Kit / Ove 2560 | FE7A | A514-5307 | 24.00M\* | 19404.40H May 5, 21 \* | 672.90H 37.51 \* | Apr 27, 23 \* | 1127.50H 53.61M\* | \* | 7.63M\* |
| **CARGO HOOK & SUSPENSION / Ove 2590     Cycle Name : HOOK TIME** | **204-072-915-103** | **HT190588** | **72.00M 1500.0C** | **19677.50H Apr 11, 22** | **185.80H** | **Apr 11, 28** | **367.30H 4.90M** | **740.60H** | **67.10M** |
| *‣ Cargo Hook / Ove 2590     Cycle Name : HOOK TIME* | *200-246-00* | *01262* | *72.00M 1500.00C* | *19677.50H Apr 11, 22  574.50C* | *559.10H 23.67  185.80C* | *Apr 20, 26  1888.70C* | *740.60H 28.57M 220.30C* | *740.60H* | *43.40M 1279.70C* |
| *‣ Load Cell / Ins 2590     Cycle Name : HOOK TIME* | *210-088-02* | *08206* | *72.00M 1500.00C* | *19677.50H Apr 11, 22* | *550.70H* | *Apr 11, 28* | *732.20H 4.90M* |  | *67.10M* |
| **Fire Bottle / Ins 2620** | **2241-009** | **67193D6** | **60.00M\*** | **18717.20H Apr 1, 19 \*** | **0.00H \*** | **Mar 25, 24 \*** | **1141.80H 41.23M\*** | **\*** | **18.57M\*** |
| *‣ Squib / Rep 2620* | *13083-45* | *00349* | *120.00M* | *18717.20H Apr 1, 19* | *0.00H 0.00* | *Apr 30, 29* | *1141.80H 41.23M* |  | *79.73M* |
| Fire Extinguisher (120 Month) / Ret 2620 | ANS429586 | BW-930843 | 120.00M | 16621.90H Apr 28, 14 |  | Apr 30, 24 | 3237.10H 100.33M |  | 19.73M |
| Fire Extinguisher (120 Month) / Ret 2620 | B417 | 741207 | 120.00M | 16270.30H Mar 31, 13 |  | Mar 31, 23 | 3588.70H 113.23M |  | 6.77M |
| Elevator (L/H) / On  2730 | 205-030-856-021 | Z-00024157 |  | 18224.60H Jan 8, 18 |  |  | 1634.40H 56.00M |  |  |
| Elevator (R/H) / On  2730 | 205-030-856-089 | ZBF-11077 |  | 18224.60H Jan 8, 18 |  |  | 1634.40H 56.00M |  |  |
| Elevator Horn / Ins 2730 | 205-001-914-107 | RE-6579 | 3000.00H | 18224.60H Jan 8, 18 | 0.00H | 21224.60H | 1634.40H 56.00M |  | 1365.60H |
| Hydraulic Accumulator / Ove 2940 | 212-076-007-003 | NES/00039 | 1000.00H | 18940.60H Nov 7, 19 | 0.00H | 19940.60H | 918.40H 34.03M |  | 81.60H |
| Hydraulic Accumulator / Ove 2940 | 212-076-007-003 | ERA5703 | 1000.00H | 18940.60H Nov 7, 19 | 0.00H | 19940.60H | 918.40H 34.03M |  | 81.60H |
| **Landing Gear /  3200** |  |  |  |  |  |  |  |  |  |
| *‣ Crosstube (AFT) / On  3200* | *212-321-104* | *1068* |  | *19677.50H Apr 11, 22* | *17142.00H* |  | *17323.50H 4.90M* | *15907.10H* |  |
| *‣ Crosstube (FWD) / Ins 3200* | *D212-664-101* | *B14477* | *300.00H 24.00M* | *19677.50H Apr 11, 22* |  | *19977.50H Apr 11, 24* | *181.50H 4.90M* |  | *118.50H 19.10M* |
| **Altimetry System / Cal 3410** |  |  | **24.00M** | **19602.70H Nov 1, 21** |  | **Nov 1, 23** | **256.30H 10.23M** |  | **13.77M** |
| *‣ Altimeter / Ins 3410* | *5934P-3* | *420261* | *24.00M* | *19602.70H Nov 1, 21* |  | *Nov 1, 23* | *256.30H 10.23M* |  | *13.77M* |
| *‣ Altimeter / Cal 3410* | *5934P-1* | *N5379* | *24.00M* | *19603.60H Dec 20, 21* |  | *Dec 20, 23* | *255.40H 8.60M* |  | *15.40M* |
| *‣ Encoder / Cal 3410* | *305154-00* | *3747* | *24.00M* | *19602.70H Nov 1, 21* |  | *Nov 1, 23* | *256.30H 10.23M* |  | *13.77M* |
| *‣ Transponder / Cal 3410* | *ATC3401-110* | *2158* | *24.00M\** | *19388.20H Apr 9, 21 \** | *\** | *Jan 28, 23 \** | *470.80H 16.97M\** | *\** | *4.67M\** |
| Compass / Cal 3420 |  |  | 12.00M | 19604.10H Jan 25, 22 |  | Jan 25, 23 | 254.90H 7.43M |  | 4.57M |
| Tailboom Assembly / On  5360 | 205-032-802-011 | AB1-00001 |  | 19678.10H Apr 13, 22 | 0.00H |  | 180.90H 4.83M | 180.90H |  |
| M/R Blade / Ret 6210 | 212-015-501-121 | BH321592 | 4000.00H | 18366.80H Apr 9, 18 | 863.40H | 21503.40H | 2355.60H 52.97M | 2355.60H | 1644.40H |
| M/R Blade / Ret 6210 | 212-015-501-121 | BH324959 | 4000.00H | 18366.80H Apr 9, 18 | 863.40H | 21503.40H | 2355.60H 52.97M | 2355.60H | 1644.40H |
| **M/R Hub Assembly / Ove 6220** | **205-812-001-103FM** | **A-61** | **2400.00H** | **19362.50H Jan 12, 21** | **0.00H** | **21762.50H** | **496.50H 19.87M** | **16585.70H** | **1903.50H** |
| *‣ Drag Brace / Ins 6220* | *204-011-140-005* | *A1-10607* | *1200.00H 24.00M* | *19362.50H Jan 12, 21* | *0.00H 0.00* | *20562.50H Jan 12, 23* | *496.50H 19.87M* |  | *703.50H 4.13M* |
| *‣ Drag Brace / Ins 6220* | *204-011-140-005* | *DI-7787* | *1200.00H 24.00M* | *19362.50H Jan 12, 21* | *0.00H 0.00* | *20562.50H Jan 12, 23* | *496.50H 19.87M* | *7492.30H* | *703.50H 4.13M* |
| *‣ Inboard Strap Fitting / Ret 6220* | *212-010-103-101* | *CQ215* | *2400.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21762.50H* | *496.50H 19.87M* | *1141.80H* | *1903.50H* |
| *‣ Inboard Strap Fitting / Ret 6220* | *212-010-103-101* | *CQ497* | *2400.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21762.50H* | *496.50H 19.87M* | *1141.80H* | *1903.50H* |
| *‣ M/R Blade Bolt Lube / Ins 6220* |  |  | *12.00M* | *19603.60H Dec 20, 21* | *0.00* | *Dec 20, 22* | *255.40H 8.60M* |  | *3.40M* |
| *‣ M/R Grip (-121) / Ret 6220* | *204-011-121-121* | *A-6066* | *25000.00H* | *19362.50H Jan 12, 21* | *2100.50H* | *42262.00H* | *2597.00H 19.87M* | *9242.50H* | *22403.00H* |
| *‣ M/R Grip (-121) / Ret 6220* | *204-011-121-121* | *A-6064* | *25000.00H* | *19362.50H Jan 12, 21* | *2100.50H* | *42262.00H* | *2597.00H 19.87M* | *9242.50H* | *22403.00H* |
| *‣ M/R Trunnion / Ret 6220     Cycle Name : RIN-X5* | *204-011-105-001* | *A-FS3891* | *15000.00H  300000.00C* | *19362.50H Jan 12, 21  358145.00C* | *5344.90H  252574.00C* | *29017.60H  405571.00C* | *5841.40H 19.87M 277769.00C* | *5841.40H  277769.00C* | *9158.60H  22231.00C* |
| *‣ M/R Yoke / Ret 6220* | *212-011-102-105* | *A-352* | *10000.00H* | *19362.50H Jan 12, 21* | *2100.50H* | *27262.00H* | *2597.00H 19.87M* | *8653.80H* | *7403.00H* |
| *‣ Outboard Strap Fitting / Ret 6220* | *204-012-103-005* | *CQ373* | *3600.00H* | *19362.50H Jan 12, 21* | *1646.60H* | *21315.90H* | *2143.10H 19.87M* | *2143.10H* | *1456.90H* |
| *‣ Outboard Strap Fitting / Ret 6220* | *204-012-103-005* | *CQ351* | *3600.00H* | *19362.50H Jan 12, 21* | *1646.60H* | *21315.90H* | *2143.10H 19.87M* | *2143.10H* | *1456.90H* |
| *‣ Pillow Block / Ins 6220* | *204-011-108-113FM* | *AERO531/97* | *2400.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21762.50H* | *496.50H 19.87M* |  | *1903.50H* |
| *‣ Pillow Block / Ins 6220* | *204-011-108-113FM* | *AERO532/97* | *2400.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21762.50H* | *496.50H 19.87M* |  | *1903.50H* |
| *‣ Pillow Block Bushing / Ret 6220* | *204-011-135-105* | *DI28178* | *3600.00H* | *19362.50H Jan 12, 21* | *0.00H* | *22962.50H* | *496.50H 19.87M* |  | *3103.50H* |
| *‣ Pillow Block Bushing / Ret 6220* | *204-011-135-105* | *DI27879* | *3600.00H* | *19362.50H Jan 12, 21* | *0.00H* | *22962.50H* | *496.50H 19.87M* |  | *3103.50H* |
| *‣ Pillow Block Bushing / Ret 6220* | *204-011-135-105* | *DI28289* | *3600.00H* | *19362.50H Jan 12, 21* | *0.00H* | *22962.50H* | *496.50H 19.87M* |  | *3103.50H* |
| *‣ Pillow Block Bushing / Ret 6220* | *204-011-135-105* | *DI28105* | *3600.00H* | *19362.50H Jan 12, 21* | *0.00H* | *22962.50H* | *496.50H 19.87M* |  | *3103.50H* |
| *‣ Pitch Horn / Ret 6220* | *204-011-120-005* | *REFS6117* | *3000.00H* | *19362.50H Jan 12, 21* | *28.30H* | *22334.20H* | *524.80H 19.87M* | *524.80H* | *2475.20H* |
| *‣ Pitch Horn / Ret 6220* | *204-011-120-005* | *REFS6138* | *3000.00H* | *19362.50H Jan 12, 21* | *28.30H* | *22334.20H* | *524.80H 19.87M* | *524.80H* | *2475.20H* |
| *‣ Strap Pin / Ret 6220* | *204-012-104-005* | *FWFS2135* | *2400.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21762.50H* | *496.50H 19.87M* | *1827.40H* | *1903.50H* |
| *‣ Strap Pin / Ret 6220* | *204-012-104-005* | *FWFS2143* | *2400.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21762.50H* | *496.50H 19.87M* | *1827.40H* | *1903.50H* |
| *‣ Strap Pin / Ret 6220* | *204-012-104-005* | *FWFS2151* | *2400.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21762.50H* | *496.50H 19.87M* | *1827.40H* | *1903.50H* |
| *‣ Strap Pin / Ret 6220* | *204-012-104-005* | *FWFS1259* | *2400.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21762.50H* | *496.50H 19.87M* | *1827.40H* | *1903.50H* |
| *‣ Tension Torsion Strap / Ret 6220* | *204-310-101-101* | *LKFS0185* | *1200.00H 24.00M* | *19362.50H Jan 12, 21* | *0.00H 0.00* | *20562.50H Jan 12, 23* | *496.50H 19.87M* | *646.20H* | *703.50H 4.13M* |
| *‣ Tension Torsion Strap / Ret 6220* | *204-310-101-101* | *LKFS0182* | *1200.00H 24.00M* | *19362.50H Jan 12, 21* | *0.00H 0.00* | *20562.50H Jan 12, 23* | *496.50H 19.87M* | *646.20H* | *703.50H 4.13M* |
| **Stab Bar Assembly / On  6220** | **212-010-300-105** | **A-662** |  | **18366.80H Apr 9, 18** | **2820.60H** |  | **4312.80H 52.97M** | **4312.80H** |  |
| *‣ Bolt (Mixing Lever Pivot (Stab. Bar (4)) / Ret 6700* | *20-057-6S24D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Stab. Bar Pivot (Stab. Bar (2)) / Ret 6700* | *20-057-10S29D* |  | *1000.00H* | *18940.60H Nov 7, 19* |  | *19940.60H* | *918.40H 34.03M* |  | *81.60H* |
| *‣ Control System Bolts (STAB BAR) / Ins 6700* | *212-704-092-001* |  | *24.00M* | *19677.20H Apr 11, 22* |  | *Apr 30, 24* | *181.80H 4.90M* |  | *19.73M* |
| *‣ M/R Pitch Link / Ret 6220* | *204-011-127-003* | *A-2444* | *9000.00H* | *18366.80H Apr 9, 18* | *6023.70H* | *21343.10H* | *7515.90H 52.97M* |  | *1484.10H* |
| *‣ M/R Pitch Link / Ret 6220* | *204-011-127-003* | *A-2438* | *9000.00H* | *18366.80H Apr 9, 18* | *6023.70H* | *21343.10H* | *7515.90H 52.97M* |  | *1484.10H* |
| *‣ Mixing Lever / Ret 6220* | *212-010-302-105* | *RE12017* | *9000.00H* | *18366.80H Apr 9, 18* | *2820.60H* | *24546.20H* | *4312.80H 52.97M* |  | *4687.20H* |
| *‣ Mixing Lever / Ret 6220* | *212-010-302-105* | *RE12011* | *9000.00H* | *18366.80H Apr 9, 18* | *2820.60H* | *24546.20H* | *4312.80H 52.97M* |  | *4687.20H* |
| *‣ Stabilizer Bar Centerframe / Ret 6220* | *204-011-307-105* | *REFS1412* | *10000.00H* | *18366.80H Apr 9, 18* | *2820.60H* | *25546.20H* | *4312.80H 52.97M* |  | *5687.20H* |
| *‣ Stabilizer Bar Centerframe / Ret 6220* | *204-011-307-105* | *REFS1442* | *10000.00H* | *18366.80H Apr 9, 18* | *2820.60H* | *25546.20H* | *4312.80H 52.97M* |  | *5687.20H* |
| *‣ Stabilizer Bar Tube / On  6220* | *212-010-311-101* | *.* |  | *18366.80H Apr 9, 18* | *2820.60H* |  | *4312.80H 52.97M* |  |  |
| *‣ Stabilizer Bar Tube / On  6220* | *212-010-311-101* | *..* |  | *18366.80H Apr 9, 18* | *2820.60H* |  | *4312.80H 52.97M* |  |  |
| Stab Bar Damper / On  6220 | 204-010-937-009 | R1900400 |  | 19826.70H Aug 19, 22 | 0.00H |  | 32.30H 0.63M |  |  |
| Stab Bar Damper / On  6220 | 204-010-937-009 | R1913209 |  | 19698.60H May 31, 22 | 349.30H 11.67 |  | 509.70H 14.90M |  |  |
| **M/R Mast Assembly (5000 Hour) / Ove 6230** | **204-040-366-021S** | **BH251779** | **5000.00H** | **18366.80H Apr 9, 18** | **897.30H** | **22469.50H** | **2389.50H 52.97M** | **2389.50H** | **2610.50H** |
| *‣ M/R Mast Bearing (5000 Hour) / On  6230* | *212-040-136-001* | *ZV13375* |  | *18366.80H Apr 9, 18* | *897.30H* |  | *2389.50H 52.97M* | *2389.50H* |  |
| *‣ Main Rotor Mast (5000 Hour) / Ret 6230     Cycle Name : RIN-X5* | *204-011-450-105* | *NFS-55901* | *15000.00H  265000.00C* | *18366.80H Apr 9, 18  315085.00C* | *897.30H  47990.00C* | *32469.50H  532095.00C* | *2389.50H 52.97M 116245.00C* | *2389.50H  116245.00C* | *12610.50H  148755.00C* |
| **Scissor & Sleeve Assembly / On  6230** | **204-011-401-021** | **RR19-0526** |  | **Nov 7, 19** |  |  | **34.03M** |  |  |
| *‣ Collective Sleeve / Ret 6710* | *204-011-408-107* | *MWFS584* | *9000.00H* | *18940.60H Nov 7, 19* | *4214.80H 14.73* | *23725.80H* | *5133.20H 48.76M* | *5133.20H* | *3866.80H* |
| *‣ Control System Bolts (SCISSOR) / Ins 6700* | *212-704-092-001* |  | *24.00M* | *19603.60H Dec 20, 21* | *0.00* | *Dec 20, 23* | *255.40H 8.60M* |  | *15.40M* |
| *‣ Scissor Assembly / On  6710* | *212-010-407-001* | *RR30-4841* |  | *18940.60H Nov 7, 19* | *13406.70H 14.73* |  | *14325.10H 48.76M* | *14325.10H* |  |
| *‣ Scissor Assembly / On  6710* | *212-010-407-001* | *RR30-5643* |  | *18940.60H Nov 7, 19* | *9781.90H 14.73* |  | *10700.30H 48.76M* | *10700.30H* |  |
| *‣ Scissors Hub / Ret 6710* | *204-011-405-013* | *EA-1377* | *9000.00H* | *18940.60H Nov 7, 19* | *4340.10H 14.73* | *23600.50H* | *5258.50H 48.76M* | *5258.50H* | *3741.50H* |
| *‣ Swashplate Drive Link / Ret 6710* | *204-011-407-001* | *RR19-7277* | *9000.00H* | *18940.60H Nov 7, 19* | *8002.10H 14.73* | *19938.50H* | *8920.50H 48.76M* | *8920.50H* | *79.50H* |
| *‣ Swashplate Drive Link / Ret 6710* | *204-011-407-001* | *RR19-7288* | *9000.00H* | *18940.60H Nov 7, 19* | *8002.10H 14.73* | *19938.50H* | *8920.50H 48.76M* | *8920.50H* | *79.50H* |
| **Swashplate & Support Assembly / On  6230** | **204-011-400-025** | **RE-0024** |  | **Nov 7, 19** |  |  | **34.03M** |  |  |
| *‣ BOLT (Coll. Lever to Swashplate (2)) / On  6700* | *AN178-22A* |  |  | *18940.60H Nov 7, 19* | *564.80H 15.63* |  | *1483.20H 49.66M* |  |  |
| *‣ Bolt (Coll. Lever to Swashplate (Swashplate (2)) / Ret 6700* | *204-011-463-107* | *PB20707* | *1000.00H* | *18940.60H Nov 7, 19* |  | *19940.60H* | *918.40H 34.03M* | *1483.20H* | *81.60H* |
| *‣ Bolt (Drivelink to Swashplate (Swashplate) / Ret 6700* | *212-010-411-005* |  | *1000.00H* | *18940.60H Nov 7, 19* | *0.00H* | *19940.60H* | *918.40H 34.03M* |  | *81.60H* |
| *‣ Bolt (Gimbal to Inner Ring) / Ret 6710* | *204-011-463-001* | *AIFS46173* | *1000.00H* | *18940.60H Nov 7, 19* |  | *19940.60H* | *918.40H 34.03M* | *1483.20H* | *81.60H* |
| *‣ Bolt (Gimbal to Inner Ring) / Ret 6710* | *204-011-463-001* | *AIFS46758* | *1000.00H* | *18940.60H Nov 7, 19* |  | *19940.60H* | *918.40H 34.03M* | *1483.20H* | *81.60H* |
| *‣ Bolt (Gimbal to Support) / Ret 6710* | *204-011-463-107* | *PB20645* | *1000.00H* | *18940.60H Nov 7, 19* |  | *19940.60H* | *918.40H 34.03M* | *1483.20H* | *81.60H* |
| *‣ Bolt (Gimbal to Support) / Ret 6710* | *20-057-8S69D* |  | *1000.00H* | *18940.60H Nov 7, 19* |  | *19940.60H* | *918.40H 34.03M* |  | *81.60H* |
| *‣ BOLT (Scissor to Drivelink (2)) / Ret 6700* | *20-057-5-30D* |  | *1000.00H* | *18940.60H Nov 7, 19* | *0.00H* | *19940.60H* | *918.40H 34.03M* |  | *81.60H* |
| *‣ COLLECTIVE LEVER / Ret 6230* | *212-010-403-005* | *FR2199* | *9000.00H* | *18940.60H Nov 7, 19* | *564.80H 14.73* | *27375.80H* | *1483.20H 48.76M* |  | *7516.80H* |
| *‣ COLLECTIVE LEVER / Ret 6230* | *212-010-403-005* | *FR2206* | *9000.00H* | *18940.60H Nov 7, 19* | *564.80H 14.73* | *27375.80H* | *1483.20H 48.76M* |  | *7516.80H* |
| *‣ Control System Bolts (Swashplate) / Ins 6700* |  |  | *24.00M* | *19603.60H Dec 20, 21* |  | *Dec 20, 23* | *255.40H 8.60M* |  | *15.40M* |
| *‣ Swashplate Gimbal Ring / Ret 6710* | *204-010-404-001* | *REFS3492* | *9000.00H* | *18940.60H Nov 7, 19* | *1472.10H 14.73* | *26468.50H* | *2390.50H 48.76M* | *2390.50H* | *6609.50H* |
| *‣ Swashplate Outer Ring / Ret 6710* | *ASI-4011-403-001* | *I-050* | *9000.00H* | *18940.60H Nov 7, 19* | *2083.30H 14.73* | *25857.30H* | *3001.70H 48.76M* | *3001.70H* | *5998.30H* |
| *‣ Swashplate Support / Ret 6710* | *204-011-404-125* | *RE20777* | *1000.00H* | *18940.60H Nov 7, 19* | *0.00H 0.00* | *19940.60H* | *918.40H 34.03M* |  | *81.60H* |
| Main Driveshaft / Ins 6310 | 205-040-004-103 | A20-2396 | 600.00H 12.00M | 19603.60H Dec 20, 21 |  | 20203.60H Dec 20, 22 | 255.40H 8.60M | 15871.90H | 344.60H 3.40M |
| **M/R Transmission Assembly / Ove 6320** | **205-040-001-049MOD** | **FH-2002** | **2000.00H** | **19362.50H Jan 12, 21** | **0.00H** | **21362.50H** | **496.50H 19.87M** | **18343.30H** | **1503.50H** |
| *‣ MGB Oil Change / Ser 6320* |  |  | *1000.00H 12.00M* | *19603.60H Dec 20, 21* | *0.00H 0.00* | *20603.60H Dec 31, 22* | *255.40H 8.60M* |  | *744.60H 3.77M* |
| *‣ MGB Oil Filter / Rep 6320* | *047546-17* |  | *1000.00H 12.00M* | *19603.60H Dec 20, 21* |  | *20603.60H Dec 31, 22* | *255.40H 8.60M* |  | *744.60H 3.77M* |
| *‣ T/R Drive Coupling (XMSN) / Ins 6520* |  |  | *600.00H 12.00M* | *19603.60H Dec 20, 21* | *0.00H 0.00* | *20203.60H Dec 31, 22* | *255.40H 8.60M* |  | *344.60H 3.77M* |
| PYLON DAMPER ASSY / On  6330 | 204-031-920-003 | LK8611 |  | 19362.50H Jan 12, 21 |  |  | 496.50H 19.87M |  |  |
| PYLON DAMPER ASSY / On  6330 | 204-031-920-003 | LK18566 |  | 19362.50H Jan 12, 21 |  |  | 496.50H 19.87M |  |  |
| **T/R Hub Assembly / Ove 6420** | **212-011-701-125** | **HNI29305** | **2500.00H** | **19362.50H Jan 12, 21** | **1448.70H** | **20413.80H** | **1945.20H 19.87M** |  | **554.80H** |
| *‣ T/R Blade / Ret 6410* | *212-010-750-133* | *A-18568* | *5000.00H* | *19362.50H Jan 12, 21* | *838.80H* | *23523.70H* | *1335.30H 19.87M* | *1335.30H* | *3664.70H* |
| *‣ T/R Blade / Ret 6410* | *212-010-750-133* | *A-18571* | *5000.00H* | *19362.50H Jan 12, 21* | *838.80H* | *23523.70H* | *1335.30H 19.87M* | *1335.30H* | *3664.70H* |
| *‣ T/R YOKE / Ret 6420* | *212-011-702-001* | *HB1484* | *5000.00H* | *19362.50H Jan 12, 21* | *3766.70H* | *20595.80H* | *4263.20H 19.87M* |  | *736.80H* |
| **T/R Hanger Assembly (G1) / Ove 6510** | **212-040-600-005** | **A20-04793** | **3000.00H** | **18224.60H Jan 8, 18** | **440.00H** | **20784.60H** | **2074.40H 56.00M** | **19606.90H** | **925.60H** |
| *‣ T/R Drive Coupling (G1) / Ins 6510* | *212-040-600-005* |  | *600.00H 12.00M* | *19603.60H Dec 20, 21* |  | *20203.60H Dec 20, 22* | *255.40H 8.60M* |  | *344.60H 3.40M* |
| **T/R Hanger Assembly (G2) / Ove 6510** | **212-040-600-005** | **A20-06679** | **3000.00H** | **18224.60H Dec 30, 99** | **390.90H** | **20833.70H** | **2025.30H** | **14329.40H** | **974.70H** |
| *‣ T/R Drive Coupling (G2) / Ins 6510* | *212-040-600-005* |  | *600.00H 12.00M* | *19603.60H Dec 20, 21* |  | *20203.60H Dec 20, 22* | *255.40H 8.60M* |  | *344.60H 3.40M* |
| **T/R Hanger Assembly (G3) / Ove 6510** | **212-040-600-101A** | **A-10964** | **3000.00H** | **18604.00H Nov 7, 18** | **1169.90H 0.23** | **20434.10H** | **2424.90H 46.26M** | **2424.90H** | **575.10H** |
| *‣ T/R Drive Coupling (G3) / Ins 6510* | *212-040-600-005* |  | *600.00H 12.00M* | *19603.60H Dec 20, 21* |  | *20203.60H Dec 20, 22* | *255.40H 8.60M* |  | *344.60H 3.40M* |
| **T/R Hanger Assembly (G4) / Ove 6510** | **212-040-600-005** | **A20-10381** | **3000.00H** | **18224.60H Jan 8, 18** | **389.90H** | **20834.70H** | **2024.30H 56.00M** | **12062.00H** | **975.70H** |
| *‣ T/R Drive Coupling (G4) / Ins 6510* | *212-040-600-005* |  | *600.00H 12.00M* | *19603.60H Dec 20, 21* |  | *20203.60H Dec 31, 22* | *255.40H 8.60M* |  | *344.60H 3.77M* |
| **Intermediate 42 Degree Gearbox / Ove 6520** | **212-040-003-023A** | **A-FS996** | **5000.00H** | **18604.00H Nov 7, 18** | **0.00H 0.03** | **23604.00H** | **1255.00H 46.06M** | **6162.50H** | **3745.00H** |
| *‣ T/R Drive Coupling (IGB) / Ins 6520* | *212-040-003-023* |  | *600.00H 12.00M* | *19603.60H Dec 20, 21* |  | *20203.60H Dec 31, 22* | *255.40H 8.60M* |  | *344.60H 3.77M* |
| **T/R 90 Degree Gearbox / Ove 6520** | **212-040-004-009** | **AFS-1125** | **5000.00H** | **17834.70H Sep 26, 16** | **2932.40H** | **19902.30H** | **4956.70H 71.40M** | **14771.40H** | **43.30H** |
| *‣ T/R Drive Coupling (TGB) / Ins 6520* |  |  | *600.00H 12.00M* | *19603.60H Dec 20, 21* |  | *20203.60H Dec 31, 22* | *255.40H 8.60M* |  | *344.60H 3.77M* |
| **Control System Bolts / Ins 6700** | **20-057-5-24D** |  | **24.00M** | **19603.60H Dec 20, 21** |  | **Dec 31, 23** | **255.40H 8.60M** |  | **15.77M** |
| *‣ Bolt (Coll. Lever to Boost Tube) / Ret 6700* | *20-057-5-22D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ BOLT (Engine Mount Pillow Block) / Rep* | *AN174-12A* |  | *1000.00H* | *19362.50H Jan 12, 21* |  | *20362.50H* | *496.50H 19.87M* |  | *503.50H* |
| *‣ Bolt (Hyd Cylinder to Lower Support) / Ret 6700* | *212-001-323-001* | *DI17370* | *2500.00H* | *18905.10H Aug 4, 19* |  | *21405.10H* | *953.90H 37.13M* |  | *1546.10H* |
| *‣ Bolt (Hyd Cylinder to Lower Support) / Ret 6700* | *212-001-323-001* | *DI17423* | *2500.00H* | *18905.10H Aug 4, 19* |  | *21405.10H* | *953.90H 37.13M* | *953.90H* | *1546.10H* |
| *‣ Bolt (Hyd Cylinder to Lower Support) / Ins 6700* | *212-001-323-001* |  | *24.00M* | *19603.60H Dec 20, 21* |  | *Dec 31, 23* | *255.40H 8.60M* |  | *15.77M* |
| *‣ Bolt (Mixing Lever to Scissors Tube) / Ret 6700* | *20-057-5-27D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Pitch Horn to Pitch Link (2)) / Ret 6700* | *20-057-6-31D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Pitch Link to Universal (2)) / Ret 6700* | *20-057-6-27D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Scissors Tube to Scissors (2)) / Ret 6700* | *20-057-5-27D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Stab. Bar Damper Tube (2)) / Ret 6700* | *AN174-15* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Stab. Bar Damper Tube (2)) / Ret 6700* | *AN174-20* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Swashplate to L/H Boost Tube) / Ret 6700* | *20-057-5-24D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Swashplate to R/H Boost Tube) / Ret 6700* | *20-057-5-24D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Universal to Boost Tube (2)) / Ret 6700* | *20-057-5-24D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Universal to Hyd. Cylinder (2)) / Ret 6700* | *20-057-5-24D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| *‣ Bolt (Universal to Mixing Lever (2)) / Ret 6700* | *20-057-6-34D* |  | *1000.00H* | *19603.60H Dec 20, 21* |  | *20603.60H* | *255.40H 8.60M* |  | *744.60H* |
| Scissors Tube / Ret 6710 | 212-010-404-005 | BHFS061877 | 9000.00H | 19603.60H Dec 20, 21 | 0.00H | 28603.60H | 255.40H 8.60M | 255.40H | 8744.60H |
| Scissors Tube / Ret 6710 | 212-010-404-005 | BHFS063025 | 9000.00H | 19015.40H Feb 22, 20 |  | 28015.40H | 843.60H 30.53M | 843.60H | 8156.40H |
| Servo, T/R / On  6720 | 212-076-004-101 | 1031 |  | 17351.80H Nov 12, 15 | 1238.80H |  | 3746.00H 81.87M |  |  |
| **T/R Controls /  6720** |  |  |  |  |  |  |  |  |  |
| *‣ Crosshead / Ove 6720* | *ASI-2010-775-001* | *E1-086* | *2500.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21862.50H* | *496.50H 19.87M* |  | *2003.50H* |
| *‣ Idler Assembly / Ove 6720* | *209-011-711-001* | *MHI-19-01* | *2500.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21862.50H* | *496.50H 19.87M* |  | *2003.50H* |
| *‣ Lever Assembly / Ove 6720* | *209-011-712-101* | *MHI-19-02* | *2500.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21862.50H* | *496.50H 19.87M* |  | *2003.50H* |
| *‣ Link Assembly / Ove 6720* | *209-011-713-003* | *MHI-09-04* | *2500.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21862.50H* | *496.50H 19.87M* |  | *2003.50H* |
| *‣ Nut, T/R Retention / Ove 6720* | *212-010-706-001* | *MHI-19-03* | *2500.00H* | *19362.50H Jan 12, 21* | *0.00H* | *21862.50H* | *496.50H 19.87M* |  | *2003.50H* |
| T/R Pitch Link / On  6720 | 212-310-701-101 |  |  | 18940.60H Nov 7, 19 |  |  | 918.40H 34.03M |  |  |
| T/R Pitch Link / On  6720 | 212-310-701-101 |  |  | 18940.60H Nov 7, 19 |  |  | 918.40H 34.03M |  |  |
| Servo, M/R / Ove 6730 | 212-076-005-111 | HR8498 | 2500.00H | 17977.60H Mar 11, 17 | 0.00H | 20477.60H | 1881.40H 65.90M | 10562.80H | 618.60H |
| Servo, M/R / Ove 6730 | 212-076-005-007 | 3493ACDFG | 2500.00H | 19603.60H Dec 20, 21 | 1726.50H 31.91 | 20377.10H | 1981.90H 40.51M | 11220.00H | 518.10H |
| Servo, M/R COL / Ove 6730 | 205-076-029-001 | 147 | 2400.00H | 17886.70H Jan 17, 17 | 0.00H | 20286.70H | 1972.30H 67.70M |  | 427.70H |
| **AFS Filter Assembly / Ins 7160** | **111300-101** |  |  | **Jul 5, 15** | **0.00** |  | **86.10M** |  |  |
| *‣ Filter Assembly / Ret 7160* | *111300-103* | *0599* | *4500.00H* | *19819.80H Aug 17, 22* |  | *24319.80H* | *39.20H 0.70M* |  | *4460.80H* |
| *‣ Filter Assembly / Ret 7160* | *111300-103* | *0254* | *4500.00H* | *19819.80H Aug 17, 22* | *2370.50H 13.24* | *21949.30H* | *2409.70H 13.94M* | *2409.70H* | *2090.30H* |
| *‣ FOD Screen / On  7160* | *111300-103* | *3197* |  | *19677.20H Apr 11, 22* |  |  | *181.80H 4.90M* | *181.80H* |  |
| *‣ FOD Screen / On  7160* | *111300-103* | *3194* |  | *19677.20H Apr 11, 22* |  |  | *181.80H 4.90M* | *181.80H* |  |
| **Engine / Ove 7200** | **1-000-060-21** | **LE07158C** | **5000.00H** | **18704.60H Mar 15, 19** |  | **23704.60H** | **1154.40H 41.77M** | **15253.10H** | **3845.60H** |
| *‣ Compressor Wash /  7200* |  |  | *100.00H* | *19856.00H Aug 27, 22* |  | *19956.00H* | *3.00H 0.37M* |  | *97.00H* |
| *‣ Engine Assembly / Ins 7200* | *1-000-060-21* |  | *2500.00H* | *18704.60H Mar 15, 19* | *0.00H* | *21204.60H* | *1154.40H 41.77M* |  | *1345.60H* |
| *‣ Engine Hot Section / Ins 7200* | *1-000-060-21* |  | *1250.00H* | *18704.60H Mar 15, 19* | *0.00H* | *19954.60H* | *1154.40H 41.77M* |  | *95.60H* |
| *‣ Fuel Control Unit / Ove 7300* | *1-170-780-01* | *02AS9309* | *2500.00H* | *19671.30H Mar 30, 22* | *1216.40H* | *20954.90H* | *1404.10H 5.27M* |  | *1095.90H* |
| *‣ Fuel Manifold / Ins 7200* | *1-130-730-02* | *OC-098-A* | *425.00H* | *19778.40H Jul 22, 22* | *0.00H 0.00* | *20203.40H* | *80.60H 1.53M* |  | *344.40H* |
| *‣ Fuel Manifold / Ins 7200* | *1-130-730-02* | *4D-152-B* | *425.00H* | *19778.40H Jul 22, 22* | *0.00H 0.00* | *20203.40H* | *80.60H 1.53M* |  | *344.40H* |
| *‣ Oil Change (Engine) / Ser 7900* |  |  | *300.00H* | *19819.80H Aug 17, 22* |  | *20119.80H* | *39.20H 0.70M* |  | *260.80H* |
| *‣ PT Governor / Ove 7250* | *1-160-850-23* | *42AM18235* | *3000.00H* | *19177.30H Aug 23, 20* | *0.00H* | *22177.30H* | *681.70H 24.50M* | *9306.80H* | *2318.30H* |
| *‣ Start Fuel Nozzle / Ins 7310* | *1-300-405-01* | *15-169016-63963* | *425.00H* | *19778.40H Jul 22, 22* |  | *20203.40H* | *80.60H 1.53M* |  | *344.40H* |
| *‣ Start Fuel Nozzle / Ins 7310* | *1-300-405-01* | *9987A* | *425.00H* | *19778.40H Jul 22, 22* |  | *20203.40H* | *80.60H 1.53M* |  | *344.40H* |
| *‣ Start Fuel Nozzle / Ins 7310* | *1-300-405-01* | *990416800888* | *425.00H* | *19778.40H Jul 22, 22* |  | *20203.40H* | *80.60H 1.53M* |  | *344.40H* |
| *‣ Start Fuel Nozzle / Ins 7310* | *1-300-405-01* | *18-169016-62641* | *425.00H* | *19778.40H Jul 22, 22* | *0.00H 0.00* | *20203.40H* | *80.60H 1.53M* |  | *344.40H* |
| HPMS Box / Cal 7700 |  |  | 12.00M | 19603.60H Dec 20, 21 |  | Dec 31, 22 | 255.40H 8.60M |  | 3.77M |
| Oil Cooler Blower / Ove 7920 | 204-062-540-001 | MHI-679 | 1000.00H | 19856.00H Aug 26, 22 | 0.00H | 20856.00H | 3.00H 0.40M |  | 997.00H |
| **Starter Generator / Ove 8000** | **30E20-61A** | **2026** | **1000.00H** | **19321.70H Oct 4, 20** | **402.50H** | **19919.20H** | **939.80H 23.13M** |  | **60.20H** |
| *‣ AD 92-27-21 Clearance Check / Ins* |  |  | *100.00H* | *19836.90H Aug 22, 22* |  | *19936.90H* | *22.10H 0.53M* |  | *77.90H* |
| *‣ Starter Generator Brush & Spline Inspection / Ins 8000* | *30E20-61A* |  | *100.00H* | *19836.90H Aug 22, 22* |  | *19936.90H* | *22.10H 0.53M* |  | *77.90H* |

" \* " indicates that a Manual Next Due is set.

| **Recurring AD's** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AD No.** | **Description** | **Type** | **Limit** | **Perf.** | **Due** | **TTSC** | **Rem.** |
| CF-91-29R1 Airframe | Annual/Installation Head Rest Insp.. | Recur | 12.00M | 19830.00H Aug 21, 22 | Aug 21, 23 | 29.00H 0.57M | 11.43M |
| AD 2022-07-02 Airframe | Vertical fin spar cap inspection. | Recur | 100.00H | 19775.10H Jul 20, 22 | 19875.10H | 83.90H 1.60M | 16.10H |
| ASB 205-15-112 Airframe | Inspection of tail rotor flight control tube and bearing. | Recur | 300.00H 12.00M | 19603.60H Dec 20, 21 | 19903.60H Dec 20, 22 | 255.40H 8.60M | 44.60H 3.40M |
| ASB 205-21-118 Airframe | Repeat inspection of tailboom attachment hardware. | Recur | 5000.00H 72.00M\* | \* | Feb 1, 22 \* | \* | -7.23M\* |
| ASB 205-17-115 (Part I) Airframe | Inspection of magnetic brake assembly P/N 204-001-376-003. | Recur | 600.00H 12.00M | 19603.60H Dec 20, 21 | 20203.60H Dec 20, 22 | 255.40H 8.60M | 344.60H 3.40M |
| AD 78-14-09 Airframe 2560 | Pyro fire warning system inspection. Engine LE07669C HUF | Recur | 100.00H | 19843.10H Aug 24, 22 | 19943.10H | 15.90H 0.47M | 84.10H |
| ASB 205-90-39 Airframe 5360 | Tailboom upper Longeron splice boroscope Inspection. Tailboom Assy. ADW-05507 | Recur | 300.00H | 19603.60H Dec 20, 21 | 19903.60H | 255.40H 8.60M | 44.60H |
| AD 2011-23-02 Airframe 6210 | Inspection of main rotor blade. | Recur | 25.00H | 19843.10H Aug 24, 22 | 19868.10H | 15.90H 0.47M | 9.10H |
| AD 2014-12-04 Pt (f)(2) Airframe 6220 | Main rotor grip tang visual inspection. M/R HUB ASSY A-61 | Recur | 25.00H | 19843.10H Aug 24, 22 | 19868.10H | 15.90H 0.47M | 9.10H |
| AD 2014-12-04 Pt (f)(4) Airframe 6220 | Main rotor grip inspection. M/R HUB ASSY A-61 | Recur | 1200.00H 24.00M | 19362.50H Jan 12, 21 | 20562.50H Jan 12, 23 | 496.50H 19.87M | 703.50H 4.13M |
| CF-88-23R1 Airframe 6220 | Main rotor pin inspection. M/R HUB ASSY A-61 | Recur | 1200.00H 24.00M | 19362.50H Jan 12, 21 | 20562.50H Jan 12, 23 | 496.50H 19.87M | 703.50H 4.13M |
| AD 2014-12-04 Pt (f)(5) Airframe 6220 | Main rotor grip inspection with blades removed. M/R HUB ASSY A-61 | Recur | 2400.00H | 19603.60H Dec 20, 21 | 22003.60H | 255.40H 8.60M | 2144.60H |
| AD 2014-12-04 (F)(3)- Part B Airframe 6220     Cycle Name : STARTS | Main rotor grip ultrasonic inspection. M/R HUB ASSY A-61 | Recur | 150.00H  600.0C | 19783.10H Aug 1, 22  12412.0C | 19933.10H  13012.0C | 75.90H 1.23M 112.0C | 74.10H  488.0C |
| CF-77-03 Airframe 6310 | Driveshaft alighnment whenever conditions of Section 7 of the  ASB exist. | Recur |  | 19603.60H Dec 20, 21 |  | 255.40H 8.60M |  |
| AD 93-17-12 Airframe 6320 | Main rotor transmission lower planetary spider MPI insp. -  NDT Bevelled Gear. M/R TRANSMISSION ASSY FH-2002 | Recur | 3100.00H | 19362.50H Jan 12, 21 | 22462.50H | 496.50H 19.87M | 2603.50H |
| AD 2013-15-02 Airframe 6410 | Inspect Tail rotor. Replaces AWD 2008-10-03. T/R HUB ASSY | Recur | 25.00H 1.00M | 19843.10H Aug 24, 22 | 19868.10H Sep 24, 22 | 15.90H 0.47M | 9.10H 0.53M |
| AD 98-11-14 Pt (c) Airframe 6420 | Tail rotor yoke inspection. T/R YOKE | Recur | 25.00H | 19843.10H Aug 24, 22 | 19868.10H | 15.90H 0.47M | 9.10H |
| AD 2001-13-01 Airframe 6420 | Tail rotor counterweight bellcrank nut and CPC. | Recur | 100.00H | 19843.10H Aug 24, 22 | 19943.10H | 15.90H 0.47M | 84.10H |
| AD 2022-10-02 Engine 7100 | Engine vibration test. Engine LE07158C | Recur | 1000.00H | 19677.90H Apr 12, 22 | 20677.90H | 181.10H 4.87M | 818.90H |
| AD 2006-11-16 Pt (h) Engine 7320 | Fuel control unit spline gear dimensional check. FUEL CONTROL UNIT | Recur | 1250.00H | 19671.30H Mar 30, 22 | 20921.30H | 187.70H 5.27M | 1062.30H |

" \* " indicates that a Manual Next Due is set.

| **Inspections** | | | | | |
| --- | --- | --- | --- | --- | --- |
| **Inspection** | **Limit** | **Perf.** | **Due** | **TTSC** | **Rem.** |
| 100 Hour Phase 1 Insp. - Form MHI 205-5 Rev. 7 | 100.00H\* | 19769.10H\* Jul 18, 22 | 19868.10H\* | 89.90H\* 1.67M | 9.10H\* |
| 100 Hour Phase 2 Insp. - Form MHI 205-10 Rev. 5 | 100.00H | 19794.10H Aug 5, 22 | 19894.10H | 64.90H 1.10M | 35.10H |
| 100 Hour Phase 3 Insp. - Form MHI 205-15 Rev. 6 | 100.00H | 19819.10H Aug 16, 22 | 19919.10H | 39.90H 0.73M | 60.10H |
| 100 Hour Phase 4 Insp. - Form MHI 205-20 Rev. 8 | 100.00H | 19843.10H Aug 24, 22 | 19943.10H | 15.90H 0.47M | 84.10H |
| 1000 Hour Insp. - Form MHI 205-25 Rev. 3 | 1000.00H | 18940.60H Nov 7, 19 | 19940.60H | 918.40H 34.03M | 81.60H |
| 300 Hour/ 12 Month Supplement Kits Insp. - Form MHI 205-35 Rev. 8 | 300.00H 12.00M | 19677.20H Apr 11, 22 | 19977.20H Apr 30, 23 | 181.80H 4.90M | 118.20H 7.73M |
| 300 Hour/12 Month Elevator Insp. - Form MHI 205-39 Rev. 3 | 300.00H 12.00M | 19603.60H Dec 20, 21 | 19903.60H Dec 31, 22 | 255.40H 8.60M | 44.60H 3.77M |
| 3000 Hour Flight Control Tube Insp. - Ref: ASB 205-76-8 | 3000.00H | 18224.60H Jan 8, 18 | 21224.60H | 1634.40H 56.00M | 1365.60H |
| 600 Hour/12 Month Elevator Insp. - Form MHI 205-40 Rev. 3 | 600.00H 12.00M | 19603.60H Dec 20, 21 | 20203.60H Dec 20, 22 | 255.40H 8.60M | 344.60H 3.40M |
| AAI 25 Hour/30 Day Skidtube Inspection | 25.00H 1.00M | 19843.10H Aug 24, 22 | 19868.10H Sep 24, 22 | 15.90H 0.47M | 9.10H 0.53M |
| M/R Tie Down Bracket Inspection. IAW MHI BM-01 | 300.00H 12.00M | 19675.60H Apr 7, 22 | 19975.60H Apr 7, 23 | 183.40H 5.03M | 116.60H 6.97M |
| Power Check | 25.00H | 19843.10H Aug 23, 22 | 19868.10H | 15.90H 0.50M | 9.10H |
| Safety Card Inspection for Placement and Correctness | 100.00H | 19797.60H Aug 8, 22 | 19897.60H | 61.40H 1.00M | 38.60H |
| 6 Month Operational Check of Crew and Passenger/Cargo Doors - Special Inspections 5-25 | 6.00M | 19778.40H Jul 25, 22 | Jan 25, 23 | 80.60H 1.43M | 4.57M |

" \* " indicates that a Manual Next Due is set.

| **Cargo Hook - Assembly - PN: 200-246-00 SN: 01262** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Cargo Hook / Ove 2590     Cycle Name : HOOK TIME | 200-246-00 | 01262 | 72.00M 1500.00C | 19677.50H Apr 11, 22  574.50C | 559.10H 23.67  185.80C | Apr 20, 26  1888.70C | 740.60H 28.57M 220.30C | 740.60H | 43.40M 1279.70C |
| -- CARGO HOOK / Ins 2590     Cycle Name : HOOK TIME | 528-020-06 |  | 12.00M 100.00C | 19677.50H Apr 11, 22 |  | Apr 11, 23 | 181.50H 4.90M |  | 7.10M |

" \* " indicates that a Manual Next Due is set.

| **Fire Extinguisher (120 Month) - Assembly - PN: ANS429586 SN: BW-930843** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Fire Extinguisher (120 Month) / Ret 2620 | ANS429586 | BW-930843 | 120.00M | 16621.90H Apr 28, 14 |  | Apr 30, 24 | 3237.10H 100.33M |  | 19.73M |
| -- Fire Extinguisher / Ins 2620 | ANS429586 |  | 12.00M | 19604.10H Jan 8, 22 |  | Jan 8, 23 | 254.90H 8.00M |  | 4.00M |

" \* " indicates that a Manual Next Due is set.

| **Fire Extinguisher (120 Month) - Assembly - PN: B417 SN: 741207** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Fire Extinguisher (120 Month) / Ret 2620 | B417 | 741207 | 120.00M | 16270.30H Mar 31, 13 |  | Mar 31, 23 | 3588.70H 113.23M |  | 6.77M |
| -- Fire Extinguisher / Ins 2620 | B417 |  | 12.00M | 19604.10H Jan 8, 22 | 0.00 | Jan 8, 23 | 254.90H 8.00M |  | 4.00M |

" \* " indicates that a Manual Next Due is set.

| **M/R Grip (-121) - Assembly - PN: 204-011-121-121 SN: A-6066** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| M/R Grip (-121) / Ret 6220 | 204-011-121-121 | A-6066 | 25000.00H | 19362.50H Jan 12, 21 | 2100.50H | 42262.00H | 2597.00H 19.87M | 9242.50H | 22403.00H |
| -- M/R GRIP (-121) / Ins 6220 | 204-011-121-121 |  | 1200.00H 24.00M | 19362.50H Jan 12, 21 | 0.00H 0.00 | 20562.50H Jan 12, 23 | 496.50H 19.87M |  | 703.50H 4.13M |

" \* " indicates that a Manual Next Due is set.

| **M/R Grip (-121) - Assembly - PN: 204-011-121-121 SN: A-6064** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| M/R Grip (-121) / Ret 6220 | 204-011-121-121 | A-6064 | 25000.00H | 19362.50H Jan 12, 21 | 2100.50H | 42262.00H | 2597.00H 19.87M | 9242.50H | 22403.00H |
| -- M/R GRIP (-121) / Ins 6220 | 204-011-121-121 |  | 1200.00H 24.00M | 19362.50H Jan 12, 21 | 0.00H 0.00 | 20562.50H Jan 12, 23 | 496.50H 19.87M |  | 703.50H 4.13M |

" \* " indicates that a Manual Next Due is set.

| **M/R Hub Assembly - Assembly - PN: 205-812-001-103FM SN: A-61** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| M/R Hub Assembly / Ove 6220 | 205-812-001-103FM | A-61 | 2400.00H | 19362.50H Jan 12, 21 | 0.00H | 21762.50H | 496.50H 19.87M | 16585.70H | 1903.50H |
| -- M/R HUB ASSY / Ins 6220 | 205-812-001-103 |  | 1200.00H 24.00M | 19362.50H Jan 12, 21 | 0.00H 0.00 | 20562.50H Jan 12, 23 | 496.50H 19.87M |  | 703.50H 4.13M |

" \* " indicates that a Manual Next Due is set.

| **M/R Yoke - Assembly - PN: 212-011-102-105 SN: A-352** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| M/R Yoke / Ret 6220 | 212-011-102-105 | A-352 | 10000.00H | 19362.50H Jan 12, 21 | 2100.50H | 27262.00H | 2597.00H 19.87M | 8653.80H | 7403.00H |
| -- M/R YOKE / Ove 6220 | 212-001-102-105 |  | 2400.00H | 19362.50H Jan 12, 21 | 0.00H | 21762.50H | 496.50H 19.87M |  | 1903.50H |
| -- M/R YOKE / Ins 6220 | 212-001-102-105 |  | 1200.00H 24.00M | 19362.50H Jan 12, 21 | 0.00H 0.00 | 20562.50H Jan 31, 23 | 496.50H 19.87M |  | 703.50H 4.77M |

" \* " indicates that a Manual Next Due is set.

| **M/R Mast Assembly (5000 Hour) - Assembly - PN: 204-040-366-021S SN: BH251779** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| M/R Mast Assembly (5000 Hour) / Ove 6230 | 204-040-366-021S | BH251779 | 5000.00H | 18366.80H Apr 9, 18 | 897.30H | 22469.50H | 2389.50H 52.97M | 2389.50H | 2610.50H |
| -- M/R MAST ASSY / Ins 6230 | 204-040-366-021S |  | 3000.00H | 18366.80H Apr 9, 18 | 897.30H 12.19 | 20469.50H | 2389.50H 65.16M |  | 610.50H |

" \* " indicates that a Manual Next Due is set.

| **T/R Hanger Assembly (G3) - Assembly - PN: 212-040-600-101A SN: A-10964** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| T/R Hanger Assembly (G3) / Ove 6510 | 212-040-600-101A | A-10964 | 3000.00H | 18604.00H Nov 7, 18 | 1169.90H 0.23 | 20434.10H | 2424.90H 46.26M | 2424.90H | 575.10H |
| -- T/R Driveshaft Bearing (G3) / Rep 6510 | 204-040-623-109 | ZS23438 | 3000.00H | 18604.00H Nov 7, 18 | 1169.90H 0.00 | 20434.10H | 2424.90H 46.03M | 2424.90H | 575.10H |

" \* " indicates that a Manual Next Due is set.

| **T/R Hanger Assembly (G1) - Assembly - PN: 212-040-600-005 SN: A20-04793** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| T/R Hanger Assembly (G1) / Ove 6510 | 212-040-600-005 | A20-04793 | 3000.00H | 18224.60H Jan 8, 18 | 440.00H | 20784.60H | 2074.40H 56.00M | 19606.90H | 925.60H |
| -- T/R Driveshaft Bearing (G1) / Rep 6510 | 204-040-623-109 | ZS31635 | 3000.00H | 18224.60H Jan 8, 18 | 440.00H | 20784.60H | 2074.40H 56.00M | 2074.40H | 925.60H |

" \* " indicates that a Manual Next Due is set.

| **T/R Hanger Assembly (G2) - Assembly - PN: 212-040-600-005 SN: A20-06679** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| T/R Hanger Assembly (G2) / Ove 6510 | 212-040-600-005 | A20-06679 | 3000.00H | 18224.60H Dec 30, 99 | 390.90H | 20833.70H | 2025.30H | 14329.40H | 974.70H |
| -- T/R Driveshaft Bearing (G2) / Ret 6510 | 204-040-632-109 | ZS29518 | 3000.00H | 18224.60H Jan 8, 18 | 390.90H | 20833.70H | 2025.30H 56.00M | 2025.30H | 974.70H |

" \* " indicates that a Manual Next Due is set.

| **T/R Hanger Assembly (G4) - Assembly - PN: 212-040-600-005 SN: A20-10381** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| T/R Hanger Assembly (G4) / Ove 6510 | 212-040-600-005 | A20-10381 | 3000.00H | 18224.60H Jan 8, 18 | 389.90H | 20834.70H | 2024.30H 56.00M | 12062.00H | 975.70H |
| -- T/R Driveshaft Bearing (G4) / Ret 6510 | 204-040-632-109 | ZS31726 | 3000.00H | 18224.60H Jan 8, 18 | 389.90H | 20834.70H | 2024.30H 56.00M | 2024.30H | 975.70H |

" \* " indicates that a Manual Next Due is set.

| **Intermediate 42 Degree Gearbox - Assembly - PN: 212-040-003-023A SN: A-FS996** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Intermediate 42 Degree Gearbox / Ove 6520 | 212-040-003-023A | A-FS996 | 5000.00H | 18604.00H Nov 7, 18 | 0.00H 0.03 | 23604.00H | 1255.00H 46.06M | 6162.50H | 3745.00H |
| -- Oil Change (42 Degree Gearbox) / Ser 6520 | 212-040-003-023 |  | 100.00H 12.00M | 19796.50H Aug 6, 22 |  | 19896.50H Aug 31, 23 | 62.50H 1.07M |  | 37.50H 11.77M |

" \* " indicates that a Manual Next Due is set.

| **T/R 90 Degree Gearbox - Assembly - PN: 212-040-004-009 SN: AFS-1125** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| T/R 90 Degree Gearbox / Ove 6520 | 212-040-004-009 | AFS-1125 | 5000.00H | 17834.70H Sep 26, 16 | 2932.40H | 19902.30H | 4956.70H 71.40M | 14771.40H | 43.30H |
| -- Oil Change (90 Degree Gearbox) / Ser 6520 | 212-040-004-009 |  | 100.00H 12.00M | 19796.50H Aug 6, 22 |  | 19896.50H Aug 6, 23 | 62.50H 1.07M |  | 37.50H 10.93M |

" \* " indicates that a Manual Next Due is set.

| **Filter Assembly - Assembly - PN: 111300-103 SN: 0599** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Filter Assembly / Ret 7160 | 111300-103 | 0599 | 4500.00H | 19819.80H Aug 17, 22 |  | 24319.80H | 39.20H 0.70M |  | 4460.80H |
| -- Filter Inspection / Ins 7160 **<< Not Installed >>** | 11300-103 |  | 300.00H 12.00M | 19819.80H Aug 17, 22 |  | 20119.80H Aug 17, 23 | 39.20H 0.70M |  | 260.80H 11.30M |

" \* " indicates that a Manual Next Due is set.

| **Filter Assembly - Assembly - PN: 111300-103 SN: 0254** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Filter Assembly / Ret 7160 | 111300-103 | 0254 | 4500.00H | 19819.80H Aug 17, 22 | 2370.50H 13.24 | 21949.30H | 2409.70H 13.94M | 2409.70H | 2090.30H |
| -- Filter Inspection / Ins 7160 | 111300-103 |  | 300.00H 12.00M | 19819.80H Aug 17, 22 |  | 20119.80H Aug 17, 23 | 39.20H 0.70M |  | 260.80H 11.30M |

" \* " indicates that a Manual Next Due is set.

| **Engine - Assembly - PN: 1-000-060-21 SN: LE07158C** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Engine / Ove 7200 \*\*Linked AD: AD 2022-10-02, AD 2009-15-13 Pt (j), AD 2009-15-13 Pt (g), AD 2006-01-05, AD 2002-15-04, AD 2002-09-09, AD 97-21-07R1, AD 97-07-05, AD 95-10-04, AD 77-17-08 R1, AD 75-22-02, AD 2022-10-02, AD 2009-15-13 Pt (j), AD 2009-15-13 Pt (g) | 1-000-060-21 | LE07158C | 5000.00H | 18704.60H Mar 15, 19 |  | 23704.60H | 1154.40H 41.77M | 15253.10H | 3845.60H |
| -- POWER SHAFT / Ret 7200     Cycle Name : PT | 1-100-800-04 | 080473300570 | 25000.00H  25000.00C | 18704.60H Mar 15, 19  4826.00C | 3459.30H 6.27  9235.00C | 40245.30H  20591.00C | 4613.70H 48.04M 12137.00C | 4613.70H  12137.00C | 20386.30H  12863.00C |
| -- CENTRIFUGAL IMPELLER / Ret 7230     Cycle Name : COMP | 1-100-078-13 | 18-162246-05467 | 15800.00H  14000.00C | 18704.60H Mar 15, 19  14415.00C | 0.00H  0.00C | 34504.60H  28415.00C | 1154.40H 41.77M 4544.00C | 6160.20H  14524.00C | 14645.60H  9456.00C |
| -- COMPRESSOR ROTOR SPOOL / Ret 7230     Cycle Name : COMP | 1-101-250-04 | MSN418748 | 12000.00H  16500.00C | 18704.60H Mar 15, 19  14415.00C | 0.00H  0.00C | 30704.60H  30915.00C | 1154.40H 41.77M 4544.00C | 11110.90H  18959.00C | 10845.60H  11956.00C |
| -- COMPRESSOR SHAFT (Front) / Ret 7230     Cycle Name : COMP | 1-100-495-07 | MSN428246 | 25000.00H  25000.00C | 18704.60H Mar 15, 19  14415.00C | 9956.50H 6.27  14415.00C | 33748.10H  25000.00C | 11110.90H 48.04M 18959.00C | 11110.90H  18959.00C | 13889.10H  6041.00C |
| -- COMPRESSOR SHAFT (Rear) / Ret 7230     Cycle Name : COMP | 1-100-501-01 | 2G059 | 25000.00H  25000.00C | 18704.60H Mar 15, 19  14415.00C | 9956.50H 6.27  14415.00C | 33748.10H  25000.00C | 11110.90H 48.04M 18959.00C | 11110.80H  18959.00C | 13889.10H  6041.00C |
| -- 1ST STAGE GP DISC / Ret 7240     Cycle Name : GP | 1-100-389-01 | 14-168522-07173 | 50000.00H  30000.00C | 18704.60H Mar 15, 19  19076.00C | 0.00H  0.00C | 68704.60H  49076.00C | 1154.40H 41.77M 4005.00C | 6180.30H  30948.70C | 48845.60H  25995.00C |
| -- 1ST STAGE GP SEALING DISC / Ret 7240     Cycle Name : GP | 1-100-399-01 | 000335703816 | 50000.00H  30000.00C | 18704.60H Mar 15, 19  19076.00C | 5005.80H 6.27  19076.00C | 63698.80H  30000.00C | 6160.20H 48.04M 23081.00C | 6160.20H  23081.00C | 43839.80H  6919.00C |
| -- 2ND STAGE GP DISC / Ret 7240     Cycle Name : GP | 1-100-397-01 | 000335701374 | 50000.00H  30000.00C | 18704.60H Mar 15, 19  19076.00C | 5005.80H 6.27  19076.00C | 63698.80H  30000.00C | 6160.20H 48.04M 23081.00C | 6160.20H  23081.00C | 43839.80H  6919.00C |
| -- 2ND STAGE GP SEALING DISC / Ret 7240     Cycle Name : GP | 1-100-379-01 | 010335702518 | 50000.00H  30000.00C | 18704.60H Mar 15, 19  19076.00C | 5005.80H 6.27  19076.00C | 63698.80H  30000.00C | 6160.20H 48.04M 23081.00C | 6160.20H  23081.00C | 43839.80H  6919.00C |
| -- GP SPACER / Ret 7240     Cycle Name : GP | 1-100-398-01 | 010335701497 | 50000.00H  30000.00C | 18704.60H Mar 15, 19  19076.00C | 5005.80H 6.27  19076.00C | 63698.80H  30000.00C | 6160.20H 48.04M 23081.00C | 6160.20H  23081.00C | 43839.80H  6919.00C |
| -- 1ST STAGE PT DISC / Ret 7250     Cycle Name : PT | 1-190-044-01 | 0916852203668 | 50000.00H  25000.00C | 18704.60H Mar 15, 19  4826.00C | 1803.00H 6.27  4826.00C | 66901.60H  25000.00C | 2957.40H 48.04M 7728.00C | 2957.40H  7728.00C | 47042.60H  17272.00C |
| -- 2ND STAGE PT DISC / Ret 7250     Cycle Name : PT | 1-140-312-01 | 020335702680 | 50000.00H  30000.00C | 18704.60H Mar 15, 19  4826.00C | 1803.00H 6.27  4826.00C | 66901.60H  30000.00C | 2957.40H 48.04M 7728.00C | 2957.40H  7728.00C | 47042.60H  22272.00C |
| -- PT SPACER / Ret 7250     Cycle Name : PT | 1-140-314-01 | 242S | 50000.00H  30000.00C | 18704.60H Mar 15, 19  4826.00C | 7972.10H 6.27  7814.00C | 60732.50H  27012.00C | 9126.50H 48.04M 10716.00C | 9126.50H  10716.00C | 40873.50H  19284.00C |

" \* " indicates that a Manual Next Due is set.

| **Fuel Control Unit - Assembly - PN: 1-170-780-01 SN: 02AS9309** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Component/Action** | **Part No.** | **Serial No.** | **Limit** | **Perf.** | **Time at Inst.** | **Due** | **TTSC** | **TTSN** | **Rem.** |
| Fuel Control Unit / Ove 7300 | 1-170-780-01 | 02AS9309 | 2500.00H | 19671.30H Mar 30, 22 | 1216.40H | 20954.90H | 1404.10H 5.27M |  | 1095.90H |
| -- FCU SILICON OIL / Ins 7300 | 1-170-780-01 |  | 1000.00H | 19671.30H Mar 30, 22 |  | 20671.30H | 187.70H 5.27M |  | 812.30H |

" \* " indicates that a Manual Next Due is set.

|  |  |  |
| --- | --- | --- |
| This report has been prepared by: | | |
|  |  |  |
| Signature | Authorization Number | Date |
| © Aircraft Maintenance Systems RD inc | | |